# Module `netapp_ontap.models.shelf_current_sensors`

Copyright © 2022 NetApp Inc. All rights reserved.

## Classes

`class ShelfCurrentSensorsSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the ShelfCurrentSensors object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `current GET POST PATCH`

    Current, in milliamps

    Example: 14410

  `id GET POST PATCH`

    The id field of the shelf_current_sensors.

    Example: 1

  `location GET POST PATCH`

    The location field of the shelf_current_sensors.

    Example: rear of the shelf on the lower left power supply

  `state GET POST PATCH`

    The state field of the shelf_current_sensors.

    Valid choices:

    - ok
    - error