# Module `netapp_ontap.models.fc_interface_svm`

Copyright © 2022 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class FcInterfaceSvmSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the FcInterfaceSvm object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `data_protocol: str GET POST`

    The data protocol for which the Fibre Channel interface is configured.

    Valid choices:

    - fcp
    - fc_nvme
  `links: SelfLink GET`

    The links field of the fc_interface_svm.

  `location: FcInterfaceSvmLocation POST`

    The location field of the fc_interface_svm.

  `name: str GET POST`

    The name of the Fibre Channel interface.

    Example: lif1

  `uuid: str GET`

    The unique identifier of the Fibre Channel interface.

    Example: 1cd8a442-86d1-11e0-ae1c-123478563412