# Module `netapp_ontap.models.storage_bridge_temperature_sensor`

Copyright © 2022 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class StorageBridgeTemperatureSensorSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the StorageBridgeTemperatureSensor object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `maximum: Size GET POST PATCH`

    Maximum safe operating temperature, in degrees Celsius.

  `minimum: Size GET POST PATCH`

    Minimum safe operating temperature, in degrees Celsius.

  `name: str GET POST PATCH`

    Temperature sensor name

    Example: Chassis temperature sensor

  `reading: Size GET POST PATCH`

    Chassis temperature sensor reading, in degrees Celsius.

  `state: str GET POST PATCH`

    The state field of the storage_bridge_temperature_sensor.

    Valid choices:

    - ok
    - warning
    - error