# Module `netapp_ontap.models.consistency_group_lun_lun_maps`

Copyright © 2022 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class ConsistencyGroupLunLunMapsSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the ConsistencyGroupLunLunMaps object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `igroup: ConsistencyGroupIgroup GET POST PATCH`

    The igroup field of the consistency_group_lun_lun_maps.

  `logical_unit_number: Size GET POST`

    The logical unit number assigned to the LUN when mapped to the specified initiator group. The number is used to identify the LUN to initiators in the initiator group when communicating through the Fibre Channel Protocol or iSCSI. Optional in POST; if no value is provided, ONTAP assigns the lowest available value.