# Module `netapp_ontap.resources.shelf`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Retrieving storage shelf information

The storage shelf GET API retrieves all of the shelves in the cluster.

## Examples

### 1) Retrieve a list of shelves from the cluster

#### The following example shows the response with a list of shelves in the cluster:

    from netapp_ontap import HostConnection
    from netapp_ontap.resources import Shelf

    with HostConnection("<mgmt-ip>", username="admin", password="password", verify=False):
        print(list(Shelf.get_collection()))

Try it out

    [
        Shelf({"uid": "3109174803597886800"}),
        Shelf({"uid": "9237728366621690448"}),
        Shelf({"uid": "9946762738829886800"}),
        Shelf({"uid": "10318311901725526608"}),
        Shelf({"uid": "13477584846688355664"}),
    ]

### 2) Retrieve a specific shelf from the cluster

#### The following example shows the response of the requested shelf. If there is no shelf with the requested uid, an error is returned.

    from netapp_ontap import HostConnection
    from netapp_ontap.resources import Shelf

    with HostConnection("<mgmt-ip>", username="admin", password="password", verify=False):
        resource = Shelf(uid=3109174803597886800)
        resource.get()
        print(resource)

Try it out

    Shelf(
        {
            "state": "ok",
            "internal": False,
            "uid": "3109174803597886800",
            "current_sensors": [
                {
                    "installed": True,
                    "current": 6990,
                    "state": "ok",
                    "id": 1,
                    "location": "rear of the shelf on the upper left power supply",
                },
                {
                    "installed": True,
                    "current": 5150,
                    "state": "ok",
                    "id": 2,
                    "location": "rear of the shelf on the upper left power supply",
                },
                {
                    "installed": True,
                    "current": 4600,
                    "state": "ok",
                    "id": 3,
                    "location": "rear of the shelf on the upper right power supply",
                },
                {
                    "installed": True,
                    "current": 4800,
                    "state": "ok",
                    "id": 4,
                    "location": "rear of the shelf on the upper right power supply",
                },
                {
                    "installed": True,
                    "current": 4140,
                    "state": "ok",
                    "id": 5,
                    "location": "rear of the shelf on the lower left power supply",
                },
                {
                    "installed": True,
                    "current": 7770,
                    "state": "ok",
                    "id": 6,
                    "location": "rear of the shelf on the lower left power supply",
                },
                {
                    "installed": True,
                    "current": 4140,
                    "state": "ok",
                    "id": 7,
                    "location": "rear of the shelf on the lower right power supply",
                },
                {
                    "installed": True,
                    "current": 4720,
                    "state": "ok",
                    "id": 8,
                    "location": "rear of the shelf on the lower right power supply",
                },
            ],
            "model": "DS4246",
            "temperature_sensors": [
                {
                    "installed": True,
                    "ambient": True,
                    "state": "ok",
                    "id": 1,
                    "temperature": 20,
                    "location": "front of the shelf on the left, on the OPS panel",
                    "threshold": {
                        "low": {"critical": 0, "warning": 5},
                        "high": {"critical": 42, "warning": 40},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 2,
                    "temperature": 29,
                    "location": "inside of the shelf on the midplane",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 55, "warning": 50},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 3,
                    "temperature": 33,
                    "location": "rear of the shelf on the upper left power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 55, "warning": 50},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 4,
                    "temperature": 41,
                    "location": "rear of the shelf on the upper left power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 70, "warning": 65},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 5,
                    "temperature": 32,
                    "location": "rear of the shelf on the upper right power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 55, "warning": 50},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 6,
                    "temperature": 41,
                    "location": "rear of the shelf on the upper right power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 70, "warning": 65},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 7,
                    "temperature": 34,
                    "location": "rear of the shelf on the lower left power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 55, "warning": 50},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 8,
                    "temperature": 45,
                    "location": "rear of the shelf on the lower left power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 70, "warning": 65},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 9,
                    "temperature": 30,
                    "location": "rear of the shelf on the lower right power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 55, "warning": 50},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 10,
                    "temperature": 40,
                    "location": "rear of the shelf on the lower right power supply",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 70, "warning": 65},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 11,
                    "temperature": 30,
                    "location": "rear of the shelf at the top left, on shelf module A",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 60, "warning": 55},
                    },
                },
                {
                    "installed": True,
                    "ambient": False,
                    "state": "ok",
                    "id": 12,
                    "temperature": 33,
                    "location": "rear of the shelf at the top right, on shelf module B",
                    "threshold": {
                        "low": {"critical": 5, "warning": 10},
                        "high": {"critical": 60, "warning": 55},
                    },
                },
            ],
            "serial_number": "SHU0954292N0HAH",
            "disk_count": 24,
            "module_type": "iom6",
            "local": True,
            "connection_type": "sas",
            "voltage_sensors": [
                {
                    "voltage": 5.11,
                    "installed": True,
                    "state": "ok",
                    "id": 1,
                    "location": "rear of the shelf on the upper left power supply",
                },
                {
                    "voltage": 12.38,
                    "installed": True,
                    "state": "ok",
                    "id": 2,
                    "location": "rear of the shelf on the upper left power supply",
                },
                {
                    "voltage": 5.11,
                    "installed": True,
                    "state": "ok",
                    "id": 3,
                    "location": "rear of the shelf on the upper right power supply",
                },
                {
                    "voltage": 12.26,
                    "installed": True,
                    "state": "ok",
                    "id": 4,
                    "location": "rear of the shelf on the upper right power supply",
                },
                {
                    "voltage": 5.7,
                    "installed": True,
                    "state": "ok",
                    "id": 5,
                    "location": "rear of the shelf on the lower left power supply",
                },
                {
                    "voltage": 12.26,
                    "installed": True,
                    "state": "ok",
                    "id": 6,
                    "location": "rear of the shelf on the lower left power supply",
                },
                {
                    "voltage": 5.15,
                    "installed": True,
                    "state": "ok",
                    "id": 7,
                    "location": "rear of the shelf on the lower right power supply",
                },
                {
                    "voltage": 12.3,
                    "installed": True,
                    "state": "ok",
                    "id": 8,
                    "location": "rear of the shelf on the lower right power supply",
                },
            ],
            "fans": [
                {
                    "installed": True,
                    "state": "ok",
                    "id": 1,
                    "location": "rear of the shelf on the upper left power supply",
                    "rpm": 3150,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 2,
                    "location": "rear of the shelf on the upper left power supply",
                    "rpm": 3000,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 3,
                    "location": "rear of the shelf on the upper right power supply",
                    "rpm": 3220,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 4,
                    "location": "rear of the shelf on the upper right power supply",
                    "rpm": 3000,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 5,
                    "location": "rear of the shelf on the lower left power supply",
                    "rpm": 3000,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 6,
                    "location": "rear of the shelf on the lower left power supply",
                    "rpm": 3150,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 7,
                    "location": "rear of the shelf on the lower right power supply",
                    "rpm": 3150,
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 8,
                    "location": "rear of the shelf on the lower right power supply",
                    "rpm": 3000,
                },
            ],
            "location_led": "off",
            "frus": [
                {
                    "installed": True,
                    "state": "ok",
                    "id": 0,
                    "firmware_version": "0191",
                    "type": "module",
                    "part_number": "111-00690+B2",
                    "serial_number": "8001900099",
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 1,
                    "firmware_version": "0191",
                    "type": "module",
                    "part_number": "111-00190+B0",
                    "serial_number": "7903785183",
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 1,
                    "firmware_version": "0311",
                    "type": "psu",
                    "psu": {"model": "9C"},
                    "part_number": "0082562-12",
                    "serial_number": "PMW82562007513E",
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 2,
                    "firmware_version": "0311",
                    "type": "psu",
                    "psu": {"model": "9C"},
                    "part_number": "0082562-12",
                    "serial_number": "PMW825620075138",
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 3,
                    "firmware_version": "0311",
                    "type": "psu",
                    "psu": {"model": "9C"},
                    "part_number": "0082562-12",
                    "serial_number": "PMW8256200750BA",
                },
                {
                    "installed": True,
                    "state": "ok",
                    "id": 4,
                    "firmware_version": "0311",
                    "type": "psu",
                    "psu": {"model": "9C"},
                    "part_number": "0082562-12",
                    "serial_number": "PMW8256200750A2",
                },
            ],
            "paths": [
                {
                    "node": {
                        "_links": {
                            "self": {
                                "href": "/api/cluster/nodes/0530d6c1-8c6d-11e8-907f-00a0985a72ee"
                            }
                        },
                        "uuid": "0530d6c1-8c6d-11e8-907f-00a0985a72ee",
                        "name": "node-1",
                    },
                    "name": "0e",
                },
                {
                    "node": {
                        "_links": {
                            "self": {
                                "href": "/api/cluster/nodes/0530d6c1-8c6d-11e8-907f-00a0985a72ee"
                            }
                        },
                        "uuid": "0530d6c1-8c6d-11e8-907f-00a0985a72ee",
                        "name": "node-1",
                    },
                    "name": "0g",
                },
            ],
            "id": "10",
            "acps": [
                {
                    "connection_state": "active",
                    "enabled": True,
                    "node": {
                        "_links": {
                            "self": {
                                "href": "/api/cluster/nodes/cf62d23c-6100-11eb-9852-00a098fd725d"
                            }
                        },
                        "uuid": "cf62d23c-6100-11eb-9852-00a098fd725d",
                        "name": "cat33-01",
                    },
                    "channel": "in_band",
                },
                {
                    "connection_state": "active",
                    "enabled": True,
                    "node": {
                        "_links": {
                            "self": {
                                "href": "/api/cluster/nodes/d0892dd7-6100-11eb-9cdb-d039ea010238"
                            }
                        },
                        "uuid": "d0892dd7-6100-11eb-9cdb-d039ea010238",
                        "name": "cat33-02",
                    },
                    "channel": "in_band",
                },
            ],
            "ports": [
                {
                    "cable": {
                        "length": "2m",
                        "serial_number": "APF16510229807",
                        "identifier": "5001086000702488-500a098000c9edbf",
                        "part_number": "112-00430+A0",
                    },
                    "designator": "square",
                    "state": "connected",
                    "id": 0,
                    "internal": False,
                    "remote": {"wwn": "5001086000702488", "phy": "08"},
                    "wwn": "500A098000C9EDBF",
                    "module_id": "a",
                },
                {
                    "cable": {
                        "length": "0.5-1.0m",
                        "serial_number": "APF133917610YT",
                        "identifier": "500a098000d5c4bf-500a098000c9edbf",
                        "part_number": "112-00176+A0",
                    },
                    "designator": "circle",
                    "state": "connected",
                    "id": 1,
                    "internal": False,
                    "remote": {"wwn": "500A098000D5C4BF", "phy": "00"},
                    "wwn": "500A098000C9EDBF",
                    "module_id": "a",
                },
                {
                    "cable": {
                        "length": "2m",
                        "serial_number": "APF16510229540",
                        "identifier": "5001086000702648-500a098004f208bf",
                        "part_number": "112-00430+A0",
                    },
                    "designator": "square",
                    "state": "connected",
                    "id": 2,
                    "internal": False,
                    "remote": {"wwn": "5001086000702648", "phy": "08"},
                    "wwn": "500A098004F208BF",
                    "module_id": "b",
                },
                {
                    "cable": {
                        "length": "0.5-1.0m",
                        "serial_number": "832210017",
                        "identifier": "500a0980062ba33f-500a098004f208bf",
                        "part_number": "112-00176+20",
                    },
                    "designator": "circle",
                    "state": "connected",
                    "id": 3,
                    "internal": False,
                    "remote": {"wwn": "500A0980062BA33F", "phy": "00"},
                    "wwn": "500A098004F208BF",
                    "module_id": "b",
                },
            ],
            "bays": [
                {"has_disk": True, "state": "ok", "id": 0, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 1, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 2, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 3, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 4, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 5, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 6, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 7, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 8, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 9, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 10, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 11, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 12, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 13, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 14, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 15, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 16, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 17, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 18, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 19, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 20, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 21, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 22, "type": "single_disk"},
                {"has_disk": True, "state": "ok", "id": 23, "type": "single_disk"},
            ],
            "name": "6.10",
            "manufacturer": {"name": "NETAPP"},
        }
    )

## Modifying storage shelf

## The storage shelf PATCH API modifies the shelf location LED.

## Example

    from netapp_ontap import HostConnection
    from netapp_ontap.resources import Shelf

    with HostConnection("<mgmt-ip>", username="admin", password="password", verify=False):
        resource = Shelf(uid=3109174803597886800)
        resource.location_led = "on"
        resource.patch()

## Classes

`class Shelf (*args, **kwargs)`

  Allows interaction with Shelf objects on the host

  Initialize the instance of the resource.

  Any keyword arguments are set on the instance as properties. For example, if the class was named 'MyResource', then this statement would be true:

      MyResource(name='foo').name == 'foo'

  ## Args

  `*args`
    Each positional argument represents a parent key as used in the URL of the object. That is, each value will be used to fill in a segment of the URL which refers to some parent object. The order of these arguments must match the order they are specified in the URL, from left to right.
  `**kwargs`
    each entry will have its key set as an attribute name on the instance and its value will be the value of that attribute.

  ### Ancestors

  - Resource

  ### Static methods

  `def count_collection (*args, connection: HostConnection = None, **kwargs) -> int`

    Returns a count of all Shelf resources that match the provided query

    This calls GET on the object to determine the number of records. It is more efficient than calling get_collection() because it will not construct any objects. Query parameters can be passed in as kwargs to determine a count of objects that match some filtered criteria.

    ## Args

    `*args`
      Each entry represents a parent key which is used to build the path to the child object. If the URL definition were /api/foos/{foo.name}/bars, then to get the count of bars for a particular foo, the foo.name value should be passed.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `**kwargs`
      Any key/value pairs passed will be sent as query parameters to the host. These query parameters can affect the count. A return_records query param will be ignored.

    ## Returns

    On success, returns an integer count of the objects of this type. On failure, returns -1.

    ## Raises

    `NetAppRestError`: If the API call returned a status code >= 400, or if there is no connection available to use either passed in or on the library.

  `def fast_get_collection (*args, connection: HostConnection = None, max_records: int = None, **kwargs) -> Iterable[RawResource]`

    Returns a list of RawResources that represent Shelf resources that match the provided query

    Fetch a list of all objects of this type from the host.

        This is a lazy fetch, making API calls only as necessary when the result
        of this call is iterated over. For instance, if max_records is set to 5,
        then iterating over the collection causes an API call to be sent to the
        server once for every 5 records. If the client stops iterating before
        getting to the 6th record, then no additional API calls are made.

    ## Args

    `*args`
      Each entry represents a parent key which is used to build the path to the child object. If the URL definition were /api/foos/{foo.name}/bars, then to get the collection of bars for a particular foo, the foo.name value should be passed.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `max_records`
      The maximum number of records to return per call
    `raw`
      return a list of `netapp_ontap.resource.RawResource` objects that require to be promoted before any RESTful operations can be used on them. Setting this argument to True makes get_collection substantially quicker when many records are returned from the server.
    `**kwargs`
      Any key/value pairs passed will be sent as query parameters to the host.

    ## Returns

    A list of `Resource` objects

    ## Raises

    `NetAppRestError`: If there is no connection available to use either passed in or on the library. This would be not be raised when get_collection() is called, but rather when the result is iterated.

  `def find (*args, connection: HostConnection = None, **kwargs) -> Resource`

    Retrieves a collection of shelves.

    ### Related ONTAP commands

    - `storage shelf show`
    - `storage shelf port show`
    - `storage shelf drawer show`
    - `storage shelf drawer show-slot`
    - `storage shelf acp show`

    ### Learn more

    - `DOC /storage/shelves`

    Find an instance of an object on the host given a query.

    The host will be queried with the provided key/value pairs to find a matching resource. If 0 are found, None will be returned. If more than 1 is found, an error will be raised or returned. If there is exactly 1 matching record, then it will be returned.

    ## Args

    `*args`
      Each entry represents a parent key which is used to build the path to the child object. If the URL definition were /api/foos/{foo.name}/bars, then to find a bar for a particular foo, the foo.name value should be passed.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `**kwargs`
      Any key/value pairs passed will be sent as query parameters to the host.

    ## Returns

    A `Resource` object containing the details of the object or None if no matches were found.

    ## Raises

    `NetAppRestError`: If the API call returned more than 1 matching resource.

  `def get_collection (*args, connection: HostConnection = None, max_records: int = None, **kwargs) -> Iterable[Resource]`

    Retrieves a collection of shelves.

    ### Related ONTAP commands

    - `storage shelf show`
    - `storage shelf port show`
    - `storage shelf drawer show`
    - `storage shelf drawer show-slot`
    - `storage shelf acp show`

    ### Learn more

    - `DOC /storage/shelves`

    Fetch a list of all objects of this type from the host.

        This is a lazy fetch, making API calls only as necessary when the result
        of this call is iterated over. For instance, if max_records is set to 5,
        then iterating over the collection causes an API call to be sent to the
        server once for every 5 records. If the client stops iterating before
        getting to the 6th record, then no additional API calls are made.

    ## Args

    `*args`
      Each entry represents a parent key which is used to build the path to the child object. If the URL definition were /api/foos/{foo.name}/bars, then to get the collection of bars for a particular foo, the foo.name value should be passed.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `max_records`
      The maximum number of records to return per call
    `raw`
      return a list of `netapp_ontap.resource.RawResource` objects that require to be promoted before any RESTful operations can be used on them. Setting this argument to True makes get_collection substantially quicker when many records are returned from the server.
    `**kwargs`
      Any key/value pairs passed will be sent as query parameters to the host.

    ## Returns

    A list of `Resource` objects

    ## Raises

    `NetAppRestError`: If there is no connection available to use either passed in or on the library. This would be not be raised when get_collection() is called, but rather when the result is iterated.

  `def patch_collection (body: dict, *args, records: Iterable[_ForwardRef('Shelf')] = None, poll: bool = True, poll_interval: Optional[int] = None, poll_timeout: Optional[int] = None, connection: HostConnection = None, **kwargs) -> NetAppResponse`

    Updates a shelf location LED.

    ### Related ONTAP commands

    - `storage shelf location-led modify`

    ### Learn more

    - `DOC /storage/shelves`

    Patch all objects in a collection which match the given query.

    All records on the host which match the query will be patched with the provided body.

    ## Args

    `body`
      A dictionary of name/value pairs to set on all matching members of the collection. The body argument will be ignored if records is provided.
    `*args`
      Each entry represents a parent key which is used to build the path to the child object. If the URL definition were /api/foos/{foo.name}/bars, then to patch the collection of bars for a particular foo, the foo.name value should be passed.
    `records`
      Can be provided in place of a query. If so, this list of objects will be patched on the host.
    `poll`
      If set to True, the call will not return until the asynchronous job on the host has completed. Has no effect if the host did not return a job response.
    `poll_interval`
      If the operation returns a job, this specifies how often to query the job for updates.
    `poll_timeout`
      If the operation returns a job, this specifies how long to continue monitoring the job's status for completion.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `**kwargs`
      Any key/value pairs passed will be sent as query parameters to the host. Only resources matching this query will be patched.

    ## Returns

    A `NetAppResponse` object containing the details of the HTTP response.

    ## Raises

    `NetAppRestError`: If the API call returned a status code >= 400

  ### Methods

  `def get (self, **kwargs) -> NetAppResponse`

    Retrieves a specific shelf.

    ### Related ONTAP commands

    - `storage shelf show`
    - `storage shelf port show`
    - `storage shelf drawer show`
    - `storage shelf drawer show-slot`
    - `storage shelf acp show`

    ### Learn more

    - `DOC /storage/shelves`

    Fetch the details of the object from the host.

    Requires the keys to be set (if any). After returning, new or changed properties from the host will be set on the instance.

    ## Returns

    A `NetAppResponse` object containing the details of the HTTP response.

    ## Raises

    `NetAppRestError`: If the API call returned a status code >= 400

  `def patch (self, hydrate: bool = False, poll: bool = True, poll_interval: Optional[int] = None, poll_timeout: Optional[int] = None, **kwargs) -> NetAppResponse`

    Updates a shelf location LED.

    ### Related ONTAP commands

    - `storage shelf location-led modify`

    ### Learn more

    - `DOC /storage/shelves`

    Send the difference in the object's state to the host as a modification request.

    Calculates the difference in the object's state since the last time we interacted with the host and sends this in the request body.

    ## Args

    `hydrate`
      If set to True, after the response is received from the call, a a GET call will be made to refresh all fields of the object.
    `poll`
      If set to True, the call will not return until the asynchronous job on the host has completed. Has no effect if the host did not return a job response.
    `poll_interval`
      If the operation returns a job, this specifies how often to query the job for updates.
    `poll_timeout`
      If the operation returns a job, this specifies how long to continue monitoring the job's status for completion.
    `connection`
      The `HostConnection` object to use for this API call. If unset, tries to use the connection which is set globally for the library or from the current context.
    `**kwargs`
      Any key/value pairs passed will normally be sent as query parameters to the host. If any of these pairs are parameters that are sent as formdata then only parameters of that type will be accepted and all others will be discarded.

    ## Returns

    A `NetAppResponse` object containing the details of the HTTP response.

    ## Raises

    `NetAppRestError`: If the API call returned a status code >= 400

  ### Inherited members

  - `Resource`:
    - `from_dict`
    - `get_collection_url`
    - `get_connection`
    - `instance_location`
    - `path_keys`
    - `poll`
    - `set_connection`
    - `to_dict`
`class ShelfSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the Shelf object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `acps: List[ShelfAcps] GET`

    Alternate Control Paths to ACP processors/functions in shelf modules and expanders

  `bays: List[ShelfBays] GET`

    The bays field of the shelf.

  `connection_type: str GET`

    The connection_type field of the shelf.

    Valid choices:

    - unknown
    - fc
    - sas
    - nvme
  `current_sensors: List[ShelfCurrentSensors] GET`

    The current_sensors field of the shelf.

  `disk_count: Size GET`

    The disk_count field of the shelf.

    Example: 12

  `drawers: List[ShelfDrawers] GET`

    The drawers field of the shelf.

  `errors: List[ShelfErrors] GET`

    The errors field of the shelf.

  `fans: List[ShelfFans] GET`

    The fans field of the shelf.

  `frus: List[ShelfFrus] GET`

    The frus field of the shelf.

  `id: str GET`

    The id field of the shelf.

    Example: 1

  `internal: bool GET`

    The internal field of the shelf.

  `local: bool GET`

    The local field of the shelf.

  `location_led: str GET PATCH`

    The location_led field of the shelf.

    Valid choices:

    - off
    - on
    - unsupported
  `manufacturer: ShelfManufacturer GET`

    The manufacturer field of the shelf.

  `model: str GET`

    The model field of the shelf.

    Example: DS2246

  `module_type: str GET`

    The module_type field of the shelf.

    Valid choices:

    - unknown
    - iom6
    - iom6e
    - iom12
    - iom12b
    - iom12c
    - iom12e
    - iom12f
    - iom12g
    - nsm100
    - nsm8e
    - nsm16e
    - psm3e
  `name: str GET`

    The name field of the shelf.

    Example: 1.1

  `paths: List[StoragePort] GET`

    The paths field of the shelf.

  `ports: List[ShelfPorts] GET`

    The ports field of the shelf.

  `serial_number: str GET`

    The serial_number field of the shelf.

    Example: SHFMS1514000895

  `state: str GET`

    The state field of the shelf.

    Valid choices:

    - unknown
    - ok
    - error
  `temperature_sensors: List[ShelfTemperatureSensors] GET`

    The temperature_sensors field of the shelf.

  `uid: str GET`

    The uid field of the shelf.

    Example: 7777841915827391056

  `vendor: ShelfVendor GET`

    The vendor field of the shelf.

  `voltage_sensors: List[ShelfVoltageSensors] GET`

    The voltage_sensors field of the shelf.