# Module `netapp_ontap.models.port_statistics_device`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class PortStatisticsDeviceSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the PortStatisticsDevice object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `link_down_count_raw: Size GET`

    The number of link state changes from up to down seen on the device.

    Example: 3

  `receive_raw: PortStatisticsPacketCounters GET`

    The receive_raw field of the port_statistics_device.

  `timestamp: ImpreciseDateTime GET`

    The timestamp when the device specific counters were collected.

    Example: 2017-01-25T11:20:13.000+0000

  `transmit_raw: PortStatisticsPacketCounters GET`

    The transmit_raw field of the port_statistics_device.