# Module `netapp_ontap.models.igroup_initiator_list_item`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class IgroupInitiatorListItemSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the IgroupInitiatorListItem object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `comment: str GET POST PATCH`

    A comment available for use by the administrator. Valid in POST and PATCH.

  `connectivity_tracking: IgroupInitiatorsConnectivityTracking GET`

    The connectivity_tracking field of the igroup_initiator_list_item.

  `igroup: Igroup GET`

    The igroup field of the igroup_initiator_list_item.

  `links: IgroupInitiatorsLinks GET`

    The links field of the igroup_initiator_list_item.

  `name: str GET POST`

    The FC WWPN, iSCSI IQN, or iSCSI EUI that identifies the host initiator. Valid in POST only and not allowed when the `records` property is used.
    An FC WWPN consists of 16 hexadecimal digits grouped as 8 pairs separated by colons. The format for an iSCSI IQN is iqn.yyyy-mm.reverse_domain_name:any. The iSCSI EUI format consists of the eui. prefix followed by 16 hexadecimal characters.

    Example: iqn.1998-01.com.corp.iscsi:name1