# Module `netapp_ontap.models.nvme_subsystem_subsystem_maps`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class NvmeSubsystemSubsystemMapsSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the NvmeSubsystemSubsystemMaps object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `anagrpid: str GET`

    The Asymmetric Namespace Access Group ID (ANAGRPID) of the NVMe namespace.
    The format for an ANAGRPIP is 8 hexadecimal digits (zero-filled) followed by a lower case "h".

    Example: 00103050h

  `links: SelfLink GET`

    The links field of the nvme_subsystem_subsystem_maps.

  `namespace: NvmeSubsystemSubsystemMapsNamespace GET POST PATCH`

    The namespace field of the nvme_subsystem_subsystem_maps.

  `nsid: str GET`

    The NVMe namespace identifier. This is an identifier used by an NVMe controller to provide access to the NVMe namespace.
    The format for an NVMe namespace identifier is 8 hexadecimal digits (zero-filled) followed by a lower case "h".

    Example: 00000001h