# Module `netapp_ontap.models.fc_switch_ports_attached_device`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class FcSwitchPortsAttachedDeviceSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the FcSwitchPortsAttachedDevice object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `port_id: str GET`

    The Fibre Channel port identifier of the attach device.

    Example: 70400

  `wwpn: str GET`

    The world-wide port name (WWPN) of the attached device.

    Example: 50:0a:21:22:23:24:25:26