# Module `netapp_ontap.models.storage_bridge_temperature_sensor`

Copyright © 2021 NetApp Inc. All rights reserved.

## Classes

`class StorageBridgeTemperatureSensorSchema (*, only: typing.Union = None, exclude: typing.Union = (), many: bool = False, context: typing.Dict = None, load_only: typing.Union = (), dump_only: typing.Union = (), partial: typing.Union = False, unknown: str = None)`

  The fields of the StorageBridgeTemperatureSensor object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `maximum GET POST PATCH`

    Maximum safe operating temperature, in degrees Celsius.

  `minimum GET POST PATCH`

    Minimum safe operating temperature, in degrees Celsius.

  `name GET POST PATCH`

    Temperature sensor name

    Example: Chassis temperature sensor

  `reading GET POST PATCH`

    Chassis temperature sensor reading, in degrees Celsius.

  `state GET POST PATCH`

    The state field of the storage_bridge_temperature_sensor.

    Valid choices:

    - ok
    - warning
    - error