# Module `netapp_ontap.models.fpolicy_engine_resiliency`

Copyright © 2022 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class FpolicyEngineResiliencySchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the FpolicyEngineResiliency object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `directory_path: str GET POST PATCH`

    Specifies the directory path under the SVM namespace, where notifications are stored in the files whenever a network outage happens.

    Example: /dir1

  `enabled: bool GET POST PATCH`

    Specifies whether the resiliency feature is enabled or not. Default is false.

  `retention_duration: str GET POST PATCH`

    Specifies the ISO-8601 duration, for which the notifications are written to files inside the storage controller during a network outage. The value for this field must be between 0 and 600 seconds. Default is 180 seconds.

    Example: PT3M