# Module `netapp_ontap.models.consistency_group_nvme_subsystem`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class ConsistencyGroupNvmeSubsystemSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the ConsistencyGroupNvmeSubsystem object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `comment: str GET POST PATCH`

    A configurable comment for the NVMe subsystem. Optional in POST and PATCH.

  `hosts: List[ConsistencyGroupNvmeHost] GET POST`

    The NVMe hosts configured for access to the NVMe subsystem. Optional in POST.

  `name: str GET POST`

    The name of the NVMe subsystem. Once created, an NVMe subsystem cannot be renamed. Required in POST.

    Example: subsystem1

  `os_type: str GET POST`

    The host operating system of the NVMe subsystem's hosts. Required in POST.

    Valid choices:

    - aix
    - linux
    - vmware
    - windows
  `uuid: str GET`

    The unique identifier of the NVMe subsystem.

    Example: 1cd8a442-86d1-11e0-ae1c-123478563412