# Module `netapp_ontap.models.shelf_frus_psu`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class ShelfFrusPsuSchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the ShelfFrusPsu object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `crest_factor: Size GET POST PATCH`

    The ratio of the peak voltage to the root-mean-square voltage

    Example: 92

  `model: str GET POST PATCH`

    The model field of the shelf_frus_psu.

    Example: 00

  `power_drawn: Size GET POST PATCH`

    Power drawn, in watts

    Example: 210

  `power_rating: Size GET POST PATCH`

    Power rating, in watts

    Example: 1600