# Module `netapp_ontap.models.ipv6_interface_and_gateway`

Copyright © 2023 NetApp Inc. All rights reserved.

This file has been automatically generated based on the ONTAP REST API documentation.

## Classes

`class Ipv6InterfaceAndGatewaySchema (*, only: Union[Sequence[str], Set[str]] = None, exclude: Union[Sequence[str], Set[str]] = (), many: bool = False, context: Dict = None, load_only: Union[Sequence[str], Set[str]] = (), dump_only: Union[Sequence[str], Set[str]] = (), partial: Union[bool, Sequence[str], Set[str]] = False, unknown: str = None)`

  The fields of the Ipv6InterfaceAndGateway object

  ### Ancestors

  - netapp_ontap.resource.ResourceSchema
  - marshmallow.schema.Schema
  - marshmallow.base.SchemaABC

  ### Class variables

  `address: str GET POST PATCH`

    IPv6 address

    Example: fd20:8b1e:b255:5011:10:141:4:97

  `gateway: str GET POST PATCH`

    The IPv6 address of the default router.

    Example: fd20:8b1e:b255:5011:10::1

  `netmask: Size GET POST PATCH`

    The IPv6 netmask/prefix length. The default value is 64 with a valid range of 1 to 127.

    Example: 64